Steering Wheel and Column Description. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

The steering column is an energy-absorbing mechanism. The steering column collapses in the event of a collision. This minimizes the possibility of injury to the driver.

The ignition switch is column-mounted. You may lock the column in order to inhibit theft. The combination switch controls the following functions:

• | The turn signal operation

• | The headlamp operation

• | The windshield wiper/washer operation

• | The cruise control operation (if equipped)

You may remove the steering column from the vehicle with relative ease. In order to ensure that the proper column energy absorption is maintained, use only the specified screws, bolts, and nuts. Tighten these fasteners to the specified torques.

Take special care in handling the column assembly if you remove the column assembly from the vehicle. The plastic injections that keep the column rigid can shear or loosen if the following events occur:

• | Using a steering wheel puller other than the recommended puller

• | Hitting the end of the steering shaft

• | Sharply leaning on the assembly

• | Dropping the assembly