Front Side Door Trim Panel Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the screw from the front side door inside handle.
2. Gently pry the front side door inside handle from the door trim panel.
3. Remove the 2 screws from the armrest (4), if equipped.
4. Remove the armrest from the door, if equipped.
5. Remove one screw from the pull handle case (1), if equipped.
6. Use a cloth in order to pull off the snap ring of the regulator handle (1).
7. Remove the regulator handle (1).
8. Gently pry the door trim panel away from the door by disengaging the retainer clips.
9. Rotate the trim panel 90 degrees counterclockwise.
10. Pull the trim panel away from the door in order to gain access to the power door electrical connector, if equipped.
11. Disconnect the power door electrical connector, if equipped.
12. Remove the door trim panel (2) from the vehicle.

### Installation Procedure

1. Position the door trim panel (2) to the door.
2. Connect the electrical connectors, if equipped.
3. Press the door trim panel plastic retainers into place.
4. Install the regulator handle (5) to the door. Secure the regulator handle (5) to the door with the snap ring.
5. Ensure the regulator handle is at a 45 degree angle when the window is fully closed.
6. Install the screw to the pull handle case, if equipped.
7. Install the armrest to the door, if equipped. Secure the armrest to the door with the 2 screws.
8. Install the front side door inside handle to the door. Secure the inside handle with the screw.