Forward Band Servo Piston Assemble. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

1. Assemble the spring seat (160) and the cushion spring (161) onto the adjusting sleeve (158).
2. Insert the adjusting sleeve (158) into the servo piston (162).
3. Place the servo piston into a press. Compress the cushion spring (161).
4. Install the cushion spring retainer ring (159).
5. Install the adjusting screw (164) into the adjusting sleeve (158).
6. Install the lock nut (165). Do not tighten the lock nut.
7. Install the piston seal ring.