Power Door Locks System Check. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 | Depress the power door lock switch to the LOCK and UNLOCK positions. | All of the doors lock and unlock. | Power Door Locks Inoperative
2 | Insert key into LH front door key lock cylinder and turn key to the counterclockwise position. | All of the doors lock. | Power Door Locks Key Lock Switch Inoperative - One
3 | Insert key into the RH front door key lock cylinder and turn key to the clockwise position. | All of the doors lock. | Power Door Locks Key Lock Switch Inoperative - One
4 | Insert key into the rear door key lock cylinder and turn key to the counterclockwise position. | All of the doors lock. | Power Door Locks Key Lock Switch Inoperative - One
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.