Rear Window Reveal Molding Replacement - Left Side. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the left-side upper and lower reveal molding joints (5, 8) from the rear door.
2. Pull the left-side reveal molding (6) from the rear door.

### Installation Procedure

Important: Trim the left-side reveal molding (6), as needed, in order to fit the left-side reveal molding (6) in the cavity between the rear door and the window.

1. Apply a bead of urethane adhesive from the kit GM P/N 12346284 into the cavity between the body and the window.
2. Install the left-side reveal molding (6).
3. Starting at the center of the left-side reveal molding (6), press the left-side reveal molding into place.
4. Press the upper and lower left-side reveal molding joints (5, 8) to the rear door.
5. Apply tape, as needed, in order to retain the left-side reveal molding (6) until the urethane cures.
6. Allow the adhesive to cure according to the manufacturer's instructions.