Power Window Inoperative - Left Side Front. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Windows System Check? | -- | Go to Step 2 | Go to Power Windows System Check

2

1. Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window motor connector from cavity 2 to ground.
2. Depress the left front window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 3

Go to Step 7

3

1. Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window motor connector from cavity 1 to ground.
2. Lift the left front window switch to the UP position.

Does the test lamp light?

--

Go to Step 4

Go to Step 9

4

1. Disconnect the left front power window motor connector.
2. Connect a J 35616-200 unpowered test lamp from cavity 2 to B+.

Does the test lamp light?

--

Go to Step 5

Go to Step 13

5 | Connect a J 35616-200 unpowered test lamp from the left front power window motor connector cavity 1 to B+. Does the test lamp light? | -- | Go to Step 6 | Go to Step 14
6 | Replace the left front power window regulator. Refer to Front Side Door Window Regulator Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --

7

1. Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window/door lock switch connector from cavity 3 to ground.
2. Depress the left front window switch to the DOWN position.

Does the test lamp light?

--

Go to Step 8

Go to Step 11

8 | Repair the open in the RED wire between the left front power window/door lock switch and the left front power window motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --

9

1. Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window/door lock switch from cavity 4 to ground.
2. Lift the left front window switch to the UP position.

Does the test lamp light?

--

Go to Step 10

Go to Step 11

10 | Repair the open in the YEL wire between the left front power window/door lock switch and the left front power window motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
11 | Use a J 35616-200 unpowered test lamp in order to backprobe the left front power door lock switch connector from cavity 10 to ground. Does the test lamp light? | -- | Go to Step 15 | Go to Step 12
12 | Repair the open in the BLU/WHT wire between the left front power window/door lock switch and fuse block 2. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Power Windows System Check | --
13 | Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window/door lock switch connector from cavity 3 to B+. Does the test lamp light? | -- | Go to Step 8 | Go to Step 15
14 | Use a J 35616-200 unpowered test lamp in order to backprobe the left front power window/door lock switch from cavity 4 to B+. Does the test lamp light? | -- | Go to Step 10 | Go to Step 15
15 | Replace the left front power window/door lock switch. Refer to Door Lock and Side Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --