Excessive Wheel Kickback or Loose Steering. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Inspect the following components and the following conditions:

• | The power steering hydraulic system for air in the lines and the reservoir

• | The steering gear for the proper and secure installation

• | The joints from the column to the steering gear for wear

• | The joints from the column to the steering gear for the proper and secure installation

• | The tie rod ends for proper and secure installation

• | The wheel bearings for wear and damage