Parking Brake Lever Bezel Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the 2 front plastic retaining clips from the parking brake lever bezel.
2. Remove the 2 rear screws.
3. Lift the parking brake bezel.
4. Disconnect the 2 electrical connectors, if equipped with power windows.
5. Remove the parking brake bezel from the vehicle.
6. Remove the power window switches from the parking brake lever bezel by squeezing the tabs on the back side of the switches, if required.

### Installation Procedure

1. Install the power window switches to the parking brake lever bezel by pushing the switches into place, if removed.
2. Connect the power window electrical connectors, if equipped.
3. Install the parking brake lever bezel to the vehicle. Secure the bezel with the 2 screws and the 2 plastic retaining clips.