LOSS OF TURN SIGNAL FUNCTION (REPL. TURN SIGNAL SWITCH). Chevrolet Beretta 1992

For 1990-2009 cars

# LOSS OF TURN SIGNAL FUNCTION (REPL. TURN SIGNAL SWITCH)

#### SUBJECT: LOSS OF TURN SIGNAL FUNCTION (REPLACE TURN SIGNAL SWITCH AND TURN SIGNAL FLASHER)

#### MODELS: 1991-94 CHEVROLET CORSICA AND BERETTA (TILT COLUMN ONLY)

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE TURN SIGNAL SWITCH MAY NOT FUNCTION.

#### CORRECTION:

REPLACE THE TURN SIGNAL SWITCH WITH P/N 19005030 THAT HAS A REDUCED QUANTITY OF GREASE AND REVISED CONTACTORS. INSTALL A NEW TURN SIGNAL FLASHER, P/N 10041073. FOR TURN SIGNAL SWITCH REPLACEMENT, REFER TO SECTION 3F5B OF THE SERVICE MANUAL. FOR TURN SIGNAL FLASHER REPLACEMENT, REFER TO SECTION 8B AND 8C OF THE SERVICE MANUAL.

PARTS ARE CURRENTLY AVAILABLE FROM GMSPO.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: N2530 (FOR TURN SIGNAL SWITCH REPLACEMENT) LABOR OPERATION NUMBER: N1760 (FOR TURN SIGNAL FLASHER REPLACEMENT) USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1994 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.