CARGO LAMP SWITCH ON WHILE REMOVING ITEMS-BATTERY DRAIN. Chevrolet Beretta 1989

For 1990-2009 cars

# CARGO LAMP SWITCH ON WHILE REMOVING ITEMS-BATTERY DRAIN

#### Model and Year: 1989 L CARS

Some owners of 1989 Corsica hatchbacks (68 style) may comment on the rear cargo lamp switch being turned on inadvertently while removing items from the rear compartment, resulting in a dead or low battery.

A new lamp and switch assembly has been released which has a guard added to protect the switch from inadvertent operation. The new lamp and switch assembly may be ordered from GMSPO, P/N 10156485. The 1990 Corsica 68 styles will have the new switch installed from start of production.

Parts are currently available from GMSPO.

Labor Operation Number: T 1513 Labor Time: .3 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.