CORRECT APPLICATION, 1/4 GLASS AND BODY LOCK PILLAR APPLIQUE. Chevrolet Beretta 1991

For 1990-2009 cars

# CORRECT APPLICATION, 1/4 GLASS AND BODY LOCK PILLAR APPLIQUE

#### Subject: CORRECT APPLICATION OF QUARTER WINDOW AND BODY LOCK PILLAR

#### Model and Year: 1991 BERETTA

When servicing the quarter window and body lock pillar applique on 1991 L coupe models, use the following VIN breakpoint information to ensure the correct parts are installed for a particular application. If a later style window is installed in a vehicle with a VIN number prior to the VIN breakpoint, an interference will occur at the upper corner between the quarter window assembly and the early style body lock pillar applique. A new applique, Body Lock Pillar, P/N 22574192 - RH, 22574193 - LH is being released to replace the early style applique P/N 101 59768 and 10 1 59769 and must be used in conjunction with the later style window on these vehicles. This new applique will provide the necessary clearance between the applique and the later style window. It may also be used with the early style window only after stock of the early style applique has been exhausted.

Prior to VIN: ME137824 (Linden Assembly Plant) MY156111 (Wilmington Assembly Plant)

Part Number Description ---------- --------------------------- 10131337 Window Assembly, Quarter - LH

10131336 Window Assembly, Quarter - RH

10159769 (22574193*) Applique, Body Lock Pillar - LH

10159768 (22574192*) Applique, Body Lock Pillar - RH

* Use only after 10159768/10159769 stock has been depleted.

Starting with VIN: ME137824 (Linden Assembly Plant) MY156111 (Wilmington Assembly Plant)

Part Number Description ------------ --------------------------- 10135529 Window Assembly, Quarter - LH 10135528 Window Assembly, Quarter - RH 22574193 Applique, Body Lock Pillar - LH 22574192 Applique, Body Lock Pillar - RH

Parts are currently available from GMSPO.

R and R Window Assembly, Quarter Labor Operation Number: C051 0 (Right Hand) C0511 (Left Hand)

R and R Applique, Body Lock Pillar Labor Operation Number: B7740 (Right Side) B7741 (Left Side)

Use applicable labor time guide for labor hours.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.