Diagnostic Trouble Code Identification. Chevrolet Beretta 1996

For 1990-2009 cars

#### Diagnostic Trouble Code (DTC) Identification Diagnostic Types

DTC | Description | DTC Type | Default Action
--- | --- | --- | ---
P0502 | Vehicle Speed Sensor (VSS) Assembly Circuit Low Input | B | DTC P0502 will be stored in PCM history
P0719 | TCC Brake Switch Circuit Low (Stuck ON) | D | DTC P0719 will be stored in PCM history
P0724 | TCC Brake Switch Circuit High (Stuck OFF) | D | DTC P0724 will be stored in PCM history
P0742 | Torque Converter Clutch (TCC) System Stuck ON | B | DTC P0742 will be stored in PCM history

P1870

Transmission Component Slipping

A

• | DTC P1870 will be stored in PCM history

• | The PCM will inhibit TCC engagement

DTC Types:

• | A - Emission related, will turn on the MIL after the first failure

• | B - Emission related, will turn on the MIL after two consecutive trips with a failure

• | C - Non-emission related, will turn on the service lamp after the first failure

• | D - Non-emission related, no lamps