Rear Compartment Lid Lock Cylinder Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Raise the rear compartment lid.
2. Remove the rear compartment lid lock cylinder retainer (4) from the lock cylinder (1).
3. Remove the rear compartment lid lock cylinder (1).

### Installation Procedure

1. Install the rear compartment lid lock cylinder (1).
2. Install the rear compartment lid lock cylinder retainer (4) to the lock cylinder (1).
3. Inspect the operation of the latch assembly.
4. Close the rear compartment lid.