Rear Seat Cushion Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Use a flat-bladed screwdriver (1) in order to press the lower rear seat cushion retainer rearward.
2. Lift the lower rear seat cushion (1) upward.
3. Remove the lower rear seat cushion (1).

### Installation Procedure

1. Install the lower rear seat cushion (1) over the brackets (2).
2. Press downward and rearward on the lower rear seat cushion (1) in order to latch the retainer (3).

Important: Pull up on cushion to insure it is retained.