Crankshaft Rear Oil Seal Installation. Chevrolet PJJ 2001

For 1990-2009 cars

#### Tools Required

J 44642 Crankshaft Rear Oil Seal Installer

1. Place the crankshaft rear oil seal onto the crankshaft.

Important: The J 44642 must be fully secured to the crankshaft to ensure proper seal depth.

2. Install the J 44642 to the crankshaft.
3. Press the crankshaft rear oil seal into position using the J 44642 . The J 44642 will bottom out when the seal reaches the proper depth.
4. Remove the J 44642 .