Power and Grounding Components. Chevrolet PJJ 2000

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Control Relay | In the left front of the engine compartment | Electrical Center Identification Views | --
Battery | In the left front of the engine compartment | -- | --
Cigar Lighter | On the console | Power and Ground Component Views | Power and Ground Connector End Views
Data Link Connector (DLC) | At the lower instrument panel tie bar | Data Link Component Views in Data Link Communications | Data Link Connector End Views in Data Link Communications
Electronic Brake Control (ABS) Relay | In the left front of the engine compartment | Electrical Center Identification Views | --
Underhood Fuse/Relay Center | In the left front of the engine compartment | Electrical Center Identification Views | --
Fuse Block | At the left end of the tie bar | Electrical Center Identification Views | --
Generator | At the right front of the engine | -- | --
Horn Relay | At the right front of the passenger compartment | Horns Component Views in Horns | Horns Connector End Views in Horns
Ignition Switch | At the right side of the steering column | Power and Ground Component Views | Power and Ground Connector End Views
Powertrain Control Module (PCM) | At the right front corner behind the fascia | Engine Controls Component Views in Engine Controls | PCM Connector End Views in Engine Controls
C100 (38 cavities) | At the left rear side of the engine compartment | Harness Routing Views | Inline Harness Connector End Views
C101 (15 cavities) | At the left rear side of the engine compartment | Harness Routing Views | Inline Harness Connector End Views
C102 (4 cavities) | At the left rear side of the engine compartment | Harness Routing Views | Inline Harness Connector End Views
C200 (23 cavities) | At the left front of the passenger compartment | Harness Routing Views | Inline Harness Connector End Views
C202 (6 cavities) | In the headliner | Harness Routing Views | Inline Harness Connector End Views
C203 (3 cavities) | In the center of the instrument panel | Harness Routing Views | Inline Harness Connector End Views
C204 (8 cavities) | At the right rear instrument panel | Harness Routing Views | Inline Harness Connector End Views
C206 (2 cavities) | At the lower instrument panel tie bar | Harness Routing Views | Inline Harness Connector End Views
C207 (2 cavities) | At the lower instrument panel tie bar | Harness Routing Views | Inline Harness Connector End Views
C220 (6 cavities) | At the left front of the passenger compartment | Harness Routing Views | Inline Harness Connector End Views
C313 (16 cavities) | On the fuel tank | Harness Routing Views | Inline Harness Connector End Views
G102 | In the left rear of the engine compartment | Harness Routing Views | --
G103 | In the left rear of the engine compartment | Harness Routing Views | --
G105 | In the left rear of the engine compartment | Harness Routing Views | --
G110 | On the left engine/transmission | Harness Routing Views | --
G112 | On the left engine/transmission | Harness Routing Views | --
G203 | On the steering column support bracket | Harness Routing Views | --
G204 | On the steering column support bracket | Harness Routing Views | --
G302 | At the right front of the passenger compartment | Harness Routing Views | --
G303 | At the right front of the passenger compartment | Harness Routing Views | --
G304 | At the left front of the passenger compartment | Harness Routing Views | --
P200 | At the left rear engine compartment in the front of the dash | -- | --
P201 | At the left lower instrument panel below the steering column | -- | --
P400 | At the rear bumper | -- | --
P500 | At the left front door to door jamb | -- | --
P600 | At the right front door to door jamb | -- | --
P700 | At the left rear door to door jamb | -- | --
P800 | At the right rear door to door jamb | -- | --
S101 (VIN 4) | In the engine harness, at the front of the engine, approximately 33 cm (13 in) from the coolant fan connector | -- | --
S101 (VIN T) | In the engine harness, at the front of the engine, approximately 28 cm (11 in) from the coolant fan connector | -- | --
S102 | In the engine harness, at the front left side of the engine, approximately 16 cm (6 in) from the engine compartment fuse/relay center | -- | --
S107 (VIN 4) | In the engine harness, at the front left side of the engine, approximately 34 cm (13 in) from the engine compartment fuse/relay center | -- | --
S107 (VIN T) | In the engine harness, at the front left side of the engine, approximately 20 cm (8 in) from the A/C compressor clutch connector | -- | --
S110 (VIN 4) | In the engine harness, at the front of the engine, approximately 20 cm (8 in) from the A/C compressor clutch connector | -- | --
S110 (VIN T) | In the engine harness, at the front of the engine, approximately 20 cm (8 in) from the A/C compressor clutch connector | -- | --
S111 (VIN 4) | In the engine harness, at the front left side of the engine, approximately 20 cm (8 in) from the A/C compressor clutch connector | -- | --
S111 (VIN T) | In the engine harness, at the front of the engine, approximately 20 cm (8 in) from the A/C compressor clutch connector | -- | --
S115 | In the forward lamp harness, approximately 50 cm (20 in) from the C101 | -- | --
S117 | In the forward lamp harness, approximately 44 cm (17 in) from C101 | -- | --
S118 | In the forward lamp harness, approximately 29 cm (11 in) from C101 | -- | --
S119 | In the forward lamp harness, approximately 33 cm (13 in) from the horn | -- | --
S121 (VIN 4) | In the engine harness, front of the engine, approximately 27 cm) (11 in) from C100 | -- | --
S121 (VIN T) | In the engine harness, front of the engine, approximately 32 cm (12.5 in) from C100 | -- | --
S122 | In the forward lamp harness, approximately 52.5 cm (21 in) from the horn connector | -- | --
S124 | In the HVAC wiring harness, approximately 78 cm (31 in) from C204 | -- | --
S125 | In the HVAC wiring harness, approximately 85 cm (33 in) from C205 | -- | --
S151 | In the forward lamp harness, approximately 12.5 cm (5 in) from C101 | -- | --
S152 | In the forward lamp harness, approximately 12.5 cm (5 in) from C101 | -- | --
S153 | In the forward lamp harness, approximately 95.5 cm (37.5 in) from C101 | -- | --
S154 | In the forward lamp harness, approximately 95.5 cm (37.5 in) from C101 | -- | --
S165 | In the fuel injector harness, approximately 29.5 cm (11.5 in) from C118 | -- | --
S171 (VIN 4) | In the engine harness, approximately 54.5 cm (21.5 in) from C100 | -- | --
S171 (VIN T) | In the engine harness, approximately 54.5 cm (21.5 in) from C101 | -- | --
S200 | In the dash harness, approximately 41.5 cm (16 in) from P201 | -- | --
S201 | In the dash harness, approximately 35 cm (14 in) from P201 | -- | --
S202 | In the dash harness, approximately 30 cm (12 in) from P201 toward the column switches | -- | --
S203 | In the dash harness, approximately 29 cm (11 in) from the electronic brake control module connector | -- | v
S204 | In the dash harness, approximately 28.5 cm (11 in) from P201 | -- | --
S205 | In the dash harness, approximately 51 cm (20 in) form P201 toward the instrument cluster connectors | -- | --
S206 | In the dash harness, approximately 21.5 cm (8.5 in) from P201 toward the instrument cluster connectors | -- | --
S207 | In the dash harness, approximately 22 cm (8.5 in) from P201 | -- | --
S209 | In the dash harness, approximately 71 cm (28 in) from P201 toward the data link connector | -- | --
S210 | In the dash harness, approximately 4 cm (1.5 in) from P201 toward the electronic brake control module connector 2 | -- | --
S211 | In the radio harness, approximately 26 cm (10 in) from C205 | -- | --
S212 | In the body harness, approximately 105 cm (41 in) from P500 | -- | --
S213 | In the dash harness, approximately 64.5 cm (24 in) from P201 toward the data link connector | -- | --
S214 | In the dash harness, approximately 18 cm (7 in) from the electronic brake control module connector 2 | -- | --
S215 | In the dash harness, approximately 85 cm (33 in) from P201 toward the sensing diagnostic module connector | -- | --
S216 | In the dash harness, approximately 15 cm (6 in) from P210 toward the instrument cluster connectors | -- | --
S217 | In the dash harness, approximately 43 cm (17 in) from P210 toward the instrument cluster connector | -- | --
S218 | In the dash harness, approximately 65.5 cm (26 in) from P201 toward the passenger inflator module connector | -- | --
S219 | In the dash harness, approximately 30 cm (12 in) from P201 toward the instrument cluster connectors | -- | --
S220 | In the dash harness, approximately 36.5 cm (14 in) from P201 toward the instrument cluster connectors | -- | --
S221 | In the dash harness, approximately 59 cm (23 in) from P201 toward the passenger inflator module connector | -- | --
S222 | In the dash harness, aproximately 47.5 cm (18.5 in) from the IP compartment lamp connector | -- | --
S223 | In the radio harness, approximately 20 cm (8 in) from C205 | -- | --
S224 | In the dash harness, approximately 72 cm (28 in) from P201 toward the passenger inflater module connector | -- | --
S225 | In the dash harness, aproximately 15.5 cm (6 in) from P201 | -- | --
S227 | In the body harness, approximately 95 cm (37 in) from P500 rearward | -- | --
S231 | IN the lamp dimmer harness, approximately 16 cm (6 in) from C201 | -- | --
S232 | In the lamp dimmer harness, approximately 19 cm (7.5 in) from the panel dimmer switch connector | -- | --
S233 | In the HVAC harness, approximately 93 cm (37 in) from C204 | -- | --
S240 | In the forward lamp harness, approximately 36.5 cm (14 in) from C101 | -- | --
S241 | In the foreword lamp harness, approximately 32.5 cm (13 in) from C102 | -- | --
S242 | In the dash harness, approximately 84 cm (33 in) fro P201 toward the data link connector | -- | --
S244 | In the forward lamp harness, approximately 56.5 (22 in) from the C101 | -- | --
S246 | In the dash harness, approximately 25.5 cm (11 in) from P201 toward the column switches | -- | --
S248 | In the body harness, approximately 62 cm (24 in) from P600 rearward | -- | --
S248 | In the body harness, approximately 38 cm (15 in) from P500 rearward | -- | --
S277 | In the dash harness, approximately 77.5 cm (30.5 in) from P201 toward the data link connector | -- | --
S280 | In the HVAC harness, approximately 58 cm (23 in) from C204 | -- | --
S281 | In the HVAC harness, approximately 98.5 cm (39 in) from C204 | -- | --
S300 | In the body harness, approximately 93 cm (37 in) from P600 rearward | -- | --
S300 (folding top) | In the body harness, approximately 102 cm (40 in) from P600 rearward | -- | --
S301 | In the body harness, approximatley 41.5 cm (16 in) from the seat belt switch connector, toward the left side of the car | -- | --
S301 (folding top) | In the body harness, approximately 50 cm (20 in) from the seat belt switch connector toward right the right side of the car | -- | --
S302 (coupe) | In the body harness, approximately 257 cm (101 in) from P500 rearward | -- | --
S303 (coupe) | In the body harness, approximately 70 cm (27.5 in) fro P600 rearward | -- | --
S303 (folding top) | In the body harness, approximately 45 cm (18 in) from P500 rearward | -- | --
S303 (sedan) | In the body harness, approximately 47 cm (18.5 in) from the park brake switch toward the right side of the car | -- | --
S304 | In the body harness, approximately 137 cm (54 in) from P500 rearward | -- | --
S305 (coupe) | In the body harness, approximately 102 cm (40 in) from the seat belt switch connector toward the left front of the car | -- | --
S305 (folding top) | In the body harness, approximately 108.5 cm (43 in) from the seat belt switch connector, toward the left side of the car | -- | --
S305 (sedan) | In the body harness, approximately 41.5 cm (16 in) from the seat belt switch connector, toward the right side of the car | -- | --
S306 | In the body harness, approximately 69 cm (27 in) from the seat belt switch connector, toward the right side of the car | -- | --
S307 | In the body harness, approximately 47 cm (18.5 in) from P500 rearward | -- | --
S330 | In the body harness, approximately 143 cm (56 in) from the left tail/stop lamp connector forward | -- | --
S331 | In the body harness, approximately 113 cm (45 in) from P600 rearward | -- | --
S332 | In the body harness, approximately 147 cm (58 in) from P500 rearward | -- | --
S350 | In the headliner harness, approximately 105 cm (41 in) from the dome lamp connector | -- | --
S351 | In the headliner harness, approximately 46 cm 918 in) from the dome lamp connector | -- | --
S352 | In the headliner harness, approximately 56 cm (22 in) from the dome lamp connector | -- | --
S353 | In the headliner harness, approximately 36 cm (14 in) from the dome lamp connector | -- | --
S371 | In the body harness, approximately 21 cm (8 in) from the folding top motor connector forward | -- | --
S372 | In the body harness, approximately 30 cm (12 in) from the folding top switch connector forward | -- | --
S400 | In the body harness, approximately 86 cm (34 in) from the left tail/stop lamp connector forward | -- | --