Engine Electrical Components. Chevrolet PJJ 2000

For 1990-2009 cars

Component | Location | Locator View | Connector End View
--- | --- | --- | ---
Battery | In the LH front of the engine compartment | -- | --
Generator | On the lower front of the engine | -- | Engine Electrical Connector End Views
Ignition Switch | On the RH side of the steering column | -- | Engine Controls Connector End Views in Engine Controls
Instrument Cluster | On the left side of the IP | Instrument Cluster Component Views in Instrument Panel Gauges and Console | Instrument Cluster Connector End Views in Instrument Panel Gauges and Console
Powertrain Control Module (PCM) | In the RH front corner behind the fascia | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Starter Motor | On the lower front of the engine | -- | --
Park/Neutral Position Switch | On the LH rear of the transmission | Automatic Transaxle Components in Automatic Transmission | Automatic Transaxle Related Connector End Views in Automatic Transmission
C100 (39 cavities) | On the LH rear of the engine cpmpartment | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G110 | On the LH rear of the transmission | Harness Routing Views in Wiring Systems | --
P201 | On the lower IP, below the steering column | Harness Routing Views in Wiring Systems | --
S202 | In the dash harness, approximately 30 cm (12 in) from P201, toward the column switches | -- | --
S277 | In the dash harness, approximately 30 cm (12 in) from P201, toward the data link connector | -- | --