Keyless Entry Components. Chevrolet PJJ 2000

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Body Control Module (BCM) | Behind the left side of the instrument panel | Body Control Module Component Views in Body Control Systems | Body Control Module Connector End Views in Body Control Systems
Body Control Module (BCM), C1 | Behind the left side of the instrument panel | Body Control Module Component Views in Body Control Systems | Body Control Module Connector End Views in Body Control Systems
Body Control Module (BCM), C2 | Behind the left side of the instrument panel | Body Control Module Component Views in Body Control Systems | Body Control Module Connector End Views in Body Control Systems
Door Lock/Unlock Relay | In the door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
IP Fuse Block | At the left end of the tie Bar | Electrical Center Identification in Wiring Systems | --
LF Door Jamb Switch | On the left front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LF Door Lock Switch | On the left front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LF Door Lock Motor | In the left front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LR Door Jamb Switch | In the left rear door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
LR Door Lock Motor | In the left rear door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Luggage Compartment Lid Release Solenoid | In the Luggage Compartment | -- | --
RF Door Jamb Switch | In the right front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RF Door Lock Switch | On the right front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RF Door Lock Motor | In the right front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RR Door Jamb Switch | In the right rear door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
RR Door Lock Motor | In the right rear door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Omron Module | On the rear package shelf | Keyless Entry Component Views | Keyless Entry Connector End Views
Programming Connector | At the left front of the luggage compartment | Keyless Entry Component Views | Keyless Entry Connector End Views
Underhood Fuse Block | In the Engine Compartment | Electrical Center Identification in Wiring Systems | --
C200 (23 Cavities) | To the left front of the passenger compartment | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C220 (6 Cavities) | To the left front of the passenger compartment | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G302 | To the right front of the passenger compartment | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
P500 | At the left front door to door jamb | -- | --
P600 | At the right front door to door jamb | -- | --
P700 | At the left rear door to door jamb | -- | --
P800 | At the right rear door to door jamb | -- | --
S303 | In the body harness approximately 255 cm (100 in) from the window switch breakout | -- | --
S307 | In the body harness approximately 47 cm (18.5 in) from P500 rearward | -- | --
S330 | In the body harness approximately 61 cm (24 in) from the OMRON Module breakout. | -- | --
S331 | In the body harness approximately 113 cm (45 in) from P600 rearward | -- | --
S390 | In the body harness approximately 5 cm (2 in) from the door lock/unlock relay. | -- | --
S391 | In the body harness approximately 78 cm (31 in) from G302 | -- | --
S392 | In the body harness approximately 22.5 cm (9 in) from the window switch breakout | -- | --
S393 | In the body harness approximately 86 cm (34 in) from G302
S902 | In the body harness approximately 90 cm (36 in) from the fuel tank pass thru grommet | -- | --