RPO Code List. Chevrolet PJJ 2000

For 1990-2009 cars

The production/process codes provide the description of the Regular Production Options (RPOs) used on the vehicle. The RPO list is printed on the Service Parts Identification Label. The following is a list of the RPO abbreviations and the description of each:

RPO | Description
--- | ---
AF5 | Easy Entry Seat Adjuster; Passenger Side
AK5 | Restraint System Front Seat, Inflatable, Driver and Passenger
AR9 | Seats; Bucket, Reclining
AS5 | Seats; Deluxe Bucket, Reclining, with Driver Lumbar Adjust, Seat Back Pocket, Firmer Side Bolsters
AU0 | Remote Keyless Entry
AU3 | Power Door Locks
C41 | HVAC, Heater System Outside Air, With Fan
C49 | Defogger, Rear Window Electric
C60 | HVAC, Air Conditioner Front Manual Controls
C95 | Lamp Interior, Roof, Courtesy and Dual Reading
DC1 | Mirror, Outside Left Hand and Right Hand Remote Control, Electric, Defog, Tinted Glass, Power, Foldaway, Painted
DC3 | Mirror, Outside Left Hand and Right Hand Remote Control, Electric, Defog, Tinted Glass, Manual Foldaway, Painted
DC4 | Mirror, Inside Rearview, Tilt, Dual Reading Lamps
DD2 | Sunvisor Vanity Mirrors
DG7 | Mirror, Outside, Remote Control, Electric, Color
DL5 | Decal Roadside Service Information
DT3 | Box Rear Storage Compartment
DT4 | Ashtray Cigarette Lighter
D35 | Mirror, Outside Remote Control, Color
FEO | Suspension System Front and Rear Active
FE1 | Suspension System, Soft Ride
FE2 | Suspension System, Ride Handling
FP2 | Ratio Transaxle Final Drive, 3.58
FX1 | Ratio Transaxle Final Drive, 3.94
FX2 | Ratio Transaxle Final Drive, 3.91
FY1 | Ratio Transaxle Final Drive, 3.63
IJC | Trim Interior Design (JC) (95)
IJN | Trim Interior Design (JN)
IPB | Trim Interior Design (PB)
IPD | Trim Interior Design (PD)
IPE | Trim Interior Design (PE)
IPG | Trim Interior Design (PG)
IPH | Trim Interior Design (PH)
IPJ | Trim Interior Design (PJ)
JA7 | Park Brake Lever Handle, Leather Wrapped
JM4 | Brake System Power, Front Disc, Rear Drum, Cast Iron, Antilock, Front and Rear Wheel
KO5 | Engine Block Heater
K29 | Module Powertrain Control
K62 | Generator, CS 130-D, 105 Amp, Dual Internal Fan
LD9 | Engine; 2.4L L4 DOHC
MN4 | Transmission, Automatic 4 Speed, 4T40E
NK5 | Steering Wheel Standard
NP5 | Steering Wheel Leather Wrapped
NW7 | Traction Control; Powertrain Mgmt Only
N33 | Stg Clm, Tilt
N46 | Steering Wheel; Deluxe Urethane, w/SIR
N78 | Wheel, 14 x 6, Aluminum, Hub Cap, Wheel Nuts
N81 | Fullsize Spare Tire
PB1 | Wheel Cover, 15 Inch
PC1 | Wheel, 14 x 6, Aluminum
PF7 | Wheel, 15 x 6, Aluminum Cast, Styled
PG1 | Wheel 14 x 6, Steel
OFB | P195/70 R14 All Season, Black Wall Tires
QPD | P195/65 R15 Touring; Black Wall Tires
QLG | P205?55 R16 Performance, Black Wall Tires
T43 | Spoiler Rear
T79 | Fog Lamp, Rear
T84 | Headlamps Right Hand Rule of the Road, E Mark
UD4 | Alarm Vehicle Speed, 120 K/H
UH7 | Cluster Instrument, Cool Temp
UH8 | Cluster Instrument, Cool Temp, Trip Odom, Tach
UJ5 | Cluster Instrument, Cool Temp, Trip Odom, Tach, Fuel, Speedo, Analog, Metric Only
UK1 | Radio, AM/FM, Stereo, Seek/Scan, Cassette and Compact Disc, Auto Tone, Clock
UQ9 | Speaker Delete
UX7 | Speaker System 4, Dual Front Door Mounted, Dual Extended Range Package Shelf
U19 | Metric Scale Instrument Cluster
U77 | Antenna Rear Window, Radio
U79 | Speakers (4), 2 Rear Shelf, 1 Coaxial per Door
VD9 | Fascia Front and Rear, Body Color
VG9 | Protector Wax, Exterior Body
VH4 | Front Mud Guards
VH9 | Envelope Owner Information Manual
VK3 | Front License Plate Mounting Provisions
VP6 | Noise Control
VR6 | Hook Tie Down
VY7 | Leather Shift Knob
V05 | Radiator Heavy Duty
01L | Secondary Color Exterior, Special (91)
10I | Interior Trim Arctic White (93)
10N | Trim Combination Vinyl, Arctic White (N) (93)
12B | Trim Combination Cloth, Graphite (B) (95)
12C | Trim Combination Cloth Graphite (C) (94)
12D | Trim Combination Cloth, Graphite (D) (95)
12E | Trim Combination Cloth, Graphite (E) (92)
12G | Trim Combination Cloth, Graphite (G) (96)
12H | Trim Combination Cloth, Graphite (H) (96)
12I | Interior Trim Graphite (95)
12J | Trim Combination Cloth, Graphite (J) (98)
16T | Top Color Bright White (94)
16U | Primary Color Exterior, Brite White (91)
22U | Primary Color Exterior, Dahlia Blue Met (97)
24U | Primary Color Exterior, Opal Blue (97)
36U | Primary Color Exterior, Fern Green Mint (99)
37U | Primary Color Exterior, Manta Green Met (96)
41T | Top Color Black (91)
41U | Primary Color Exterior, Black (94)
49U | Primary Color Exterior, Light Sandrift Met (96)
52B | Trim Combination Cloth, Light Neutral (B) (92)
52C | Trim Combination Cloth, Light Neutral (C) (95)
52D | Trim Combination Cloth, Light Neutral (D) (96)
52E | Trim Combination Cloth, Light Neutral (E) (96)
52G | Trim Combination Cloth, Light Neutral (G) (96)
52H | Trim Combination Cloth, Medium Neutral II (H) (96)
52I | Interior Trim, Light Neutral (I) (92)
52N | Trim Combination Vinyl, Light Neutral (N) (96)
52T | Top Color Neutral
6OU | Primary Color Exterior, Gold Firemist (98)
8X1 | Label Fastener Seat Belts
81U | Primary Color Exterior, Bright Red (91)
92B | Trim Combination Cloth, Pewter (B) (97)
92E | Trim Combination Cloth, Medium Dark Pewter (97) (E)
92G | Trim Combination Cloth, Medium Dark Pewter (97) (G)
92H | Trim Combination Cloth, Medium Dark Pewter (97) (H)
92I | Interior Trim Pewter (97)
96U | Primary Color Exterior, Cayenne Red Metallic (96)