Brake Warning System Check. Chevrolet PJJ 2000

For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---

1

1. Turn the ignition switch to the RUN position.
2. Park brake not applied.

BRAKE indicator Illuminates briefly then turns off.

Brake Warning Indicator Always On

Brake Warning Indicator Inoperative

2 | Apply the park brake. | BRAKE indicator Illuminates. | Brake Warning Indicator Inoperative
3 | Brake fluid level low. | BRAKE indicator Illuminates. | Brake Warning Indicator Inoperative
* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.