Approximate Fluid Capacities. Chevrolet PJJ 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Cooling System

- Engine Cooling, 2.4L

10.1 L

10.7 qt

Engine Crankcase

- With Filter

3.8 L

4.0 qt

Fuel System

- Fuel Tank

56.8 gal

15 gal

Transaxle

- 4T40E/4T45E Transaxle (Bottom Pan Removal)

6.5 L

6.9 qt

- 4T40E/4T45E Transaxle (Complete Overhaul)

9 L

9.5 qt

- 4T40E/4T45E Transaxle (Dry)

12.2 L

12.9 qt