Rear Compartment Lid Adjustment. Chevrolet PJJ 2001

For 1990-2009 cars

### Adjustment Procedure

You may adjust the rear compartment lid using one of the following methods.

#### Procedure A:

1. Loosen the compartment lid hinge bolts. Refer to Compartment Lid Replacement - Rear.
2. Adjust the compartment lid clearance.
3. Tighten the compartment lid hinge bolts. Refer to Compartment Lid Replacement - Rear.

#### Procedure B:

1. Remove the rear window trim panel. Refer to Trim Panel Replacement - Rear Window.
2. Loosen the compartment lid hinge bolts at the rear window panel. Refer to Compartment Lid Replacement - Rear.
3. Adjust the compartment lid clearance.
4. Tighten the compartment lid hinge bolts at the rear window panel. Refer to Compartment Lid Replacement - Rear.
5. Install the rear window trim panel. Refer to Compartment Lid Replacement - Rear.