Power Brake Booster Vacuum Hose Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Disconnect the vacuum brake booster hose (3) from the vacuum brake booster check valve (2).
2. Disconnect the vacuum brake booster hose (3) from the vacuum pipe (6).
3. Remove the vacuum brake booster hose (3) from the vehicle.

### Installation Procedure

1. Install the vacuum brake booster hose (3) to the vehicle.
2. Connect the vacuum brake booster hose (3) to the vacuum pipe (6).
3. Connect the vacuum brake booster hose (3) to the vacuum brake booster check valve (2).