Radio Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Disable the SIR system. Refer to Disabling the SIR System in SIR.
2. Remove the IP cluster trim plate. Refer to Trim Plate Bezel Replacement - IP Cluster in Instrument Panel, Gauges and Console.
3. Remove the screws (1).
4. Pull the radio (2) out from the instrument panel (3).
5. Disconnect the electrical connections.
6. Disconnect the antenna lead connections.
7. Remove the radio (2) from the vehicle.

### Installation Procedure

1. Connect the electrical connections to the radio (2).
2. Connect the antenna lead connections to the radio.
3. Install the radio (2) to the instrument panel (3).
4. Install the screws (1) to the instrument panel.
5. Install the IP cluster trim plate. Refer to Trim Plate Bezel Replacement - IP Cluster in Instrument Panel, Gauges and Console.
6. Enable the SIR system. Refer to Enabling the SIR System in SIR.