Front Seat Cushion Cover Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the driver or passenger front seat. Refer to Seat Replacement.
2. Place the front seat on a clean, dry, non - abrasive surface.
3. Remove the front seat back from the seat cushion. Refer to Seat Back Replacement - Front.
4. Remove the seat pad and cover J-retainers (1) from the seat cushion frame (2).
5. Remove the seat pad and cover assembly (1) from the seat frame (3).

### Installation Procedure

1. Install the seat pad and cover assembly (1) to the seat frame (3).
2. Install the seat pad and cover J-retainers (2) to the seat frame.
3. Install the front seat back to the seat cushion. Refer to Seat Back Replacement - Front.
4. Install the driver or passenger front seat. Refer to Seat Replacement.