Center Pillar Garnish Molding Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the seat retractor side belt.
2. Pull the center pillar upper trim panel outward at the roof in order to disengage the clips.
3. Pull the center pillar upper trim panel (1) upward in order to disengage the panel from the carpet.

### Installation Procedure

1. Insert the center pillar upper trim panel (1) into the retainer.
2. Push the center pillar upper trim panel (1) in order to engage the clips.
3. Install the front seat retractor side belt.