Power Door Systems Component Views. Chevrolet PJJ 2000

For 1990-2009 cars

Figure 1:

#### Cigar Lighter

(1) | Hazard Switch
(2) | Outside Mirror Switch
(3) | Fog Lamp Switch
(4) | Cigar Lighter

Figure 2:

#### LR Door

(1) | Door Lock Motor -- LR Connector
(2) | Window Motor -- LR Connector
(3) | Window Switch -- LR Connector
(4) | Door Jamb Switch -- LR Connector

Figure 3:

#### Master Window Switch Lead

(1) | Master Window Switch
(2) | Power Window Switch Lead

Figure 4:

#### RF, LR and LF Door Jamb Switch Connector

(1) | Door Jamb Switch Connector, Front Passenger
(2) | Door Jamb Switch, Front Passenger
(3) | Door Jamb Switch, Left Rear LR
(4) | Door Jamb Switch Connector, LR
(5) | Door Jamb Switch, Driver
(6) | Door Jamb Switch Connector, Driver

Figure 5:

#### Right Front I/P Compartment

(1) | Door Lock Relay
(2) | Door Jamb Connector, Front Passenger
(3) | HVAC Connector
(4) | Antenna Lead
(5) | Radio Connector

Figure 6:

#### Inside the Door Panel

(1) | Power Mirror Connector
(2) | Speaker Connector
(3) | Power Door Lock Switch Connector
(4) | Power Window Motor and Connector

Figure 7:

#### Behind the Driver Side Kick Panel

(1) | Foldaway Mirror Module
(2) | Power Door Lock/Unlock Relay
(3) | Power Window Control Module (Express)