Fastener Tightening Specifications. Chevrolet PJJ 2001

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Fuel Tank Filler Door Nut | 2.8 N·m | 24.8 lb in
Fuel Tank Filler Pocket Bolt | Fully Driven, Seated, Not Stripped
Rear Compartment Deck Lid Spoiler Nut | 5 N·m | 44 lb in
Rear Compartment Lid Applique Nut | 3 N·m | 27 lb in
Rear Compartment Lid Applique Nut (Pontiac Coupe) | 5 N·m | 44 lb in
Rear Compartment Lid Hinge Bolt to Rear Compartment Lid | 7 N·m | 62 lb in
Rear Compartment Lid Hinge Nut | 12 N·m | 9 lb ft
Rear Compartment Lid Hinge Bolt to Rear Window Panel | 10 N·m | 89 lb in
Rear Compartment Lid Latch Assembly Bolt | 6 N·m | 53 lb in
Rear Compartment Lid Lock Striker Nut | 10 N·m | 89 lb in
Rear Compartment Lid Remote Release Handle Screw | 1 N·m | 12 lb in
Rear Compartment Lid Spoiler Bolt (Chevrolet) | 5 N·m | 44 lb in
Tail Lamp Filler Nut | 6 N·m | 53 lb in