Driver or Passenger Seat Back Cushion Cover and Pad Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the headrest. Refer to Front Seat Head Restraint Replacement
2. Remove the knob from the release lever on the seat back lock on Coupe and Convertible models.
3. Disconnect the closeout strip (1).
4. Remove the seat back pad (2) and cover (1).

### Installation Procedure

1. Install the seat back pad (2) and cover (1).
2. Reconnect the closeout strip (1).
3. Install the knob for the release lever on the seat back lock.
4. Install the headrest. Refer to Front Seat Head Restraint Replacement

Important: Care must be used on seats with maps pockets, so that the card board backing from old seat must be used in new seat or seat appearance will be distorted.

5. Reconnect back to cushion.