Diagnostic Trouble Code (DTC) List. Chevrolet PJJ 2000

For 1990-2009 cars

Description | Module
--- | ---
DTC U1000 Class 2 Communication Malfunction | BCM, PCM, IPC, SDM, EBCM, Radio
DTC U1016 Loss of Communications with PCM | BCM, IPC, SDM, EBCM, Radio
DTC U1040 Loss of Class 2 Communications with ABS | BCM, PCM, IPC, SDM, Radio
DTC U1064 Loss of Communications with BCM | PCM, IPC, SDM, EBCM, Radio
DTC U1088 Loss of Communications with SDM | BCM, PCM, IPC, EBCM, Radio
DTC U1096 Loss of Communications with IPC | BCM, PCM, SDM, EBCM, Radio
DTC U1128 Loss of Communications with RADIO | BCM, PCM, IPC, SDM, EBCM
DTC U1300 Class 2 Data Link Low | PCM, SDM, EBCM, Radio
DTC U1301 Class 2 Data Link High | PCM, SDM, EBCM, Radio