HARD START, ROUGH RUN, ACCEL. FUEL ADDITIVE FOR INJECTORS. Pontiac 6000 1987

For 1990-2009 cars

# HARD START, ROUGH RUN, ACCEL. FUEL ADDITIVE FOR INJECTORS

ALL MODELS WITH MPFI ENGINES

Some Pontiacs may experience a condition of hard starting, rough running, or poor acceleration due to restricted fuel injectors. General Motors Parts is now marketing a fuel additive detergent to help prevent deposit build up on fuel injectors. The additive part number is 12345104.

SERVICE DEPARTMENT PONTIAC DIVISION GENERAL MOTORS CORPORATION

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.