SIX-WAY MANUAL SEAT NEW RETAINER BUSHING. Pontiac 6000 1984

For 1990-2009 cars

# SIX-WAY MANUAL SEAT NEW RETAINER BUSHING

To reduce up-down (rocking) movement between the two front plate assembly retaining pins a new retainer bushing (20437151) (white in color) has been released for service.

When installing the new bushing, the bushing flange (see illustration) must be located as shown.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.