EXHAUST SYSTEM RATTLE PARK BRAKE CABLE CONTACT. Pontiac Fiero 1984

For 1990-2009 cars

# EXHAUST SYSTEM RATTLE PARK BRAKE CABLE CONTACT

ALL 1984 THRU 1986 FIERO MODELS

Some 1984 thru 1986 Fieros may exhibit a rattle noise from the left rear of the vehicle. If a rattle exists, check for interference between the front park brake cable and the exhaust system (left rear tailpipe)

If interference is present, install an "S" clip between the front and left brake cables as shown in the illustration.

Service P/N 10046461

Labor Operation: T3152

Labor Time 0.2 hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.