INSTRUMENT PANEL CLUSTER REPAIR- V6 ENGINE. Pontiac Fiero 1986

For 1990-2009 cars

# INSTRUMENT PANEL CLUSTER REPAIR- V6 ENGINE

1986 FIERO

#### CONDITION:

---------- On some 1986 Fiero models, the odometer will not register additional mileage or the 10 amp gage fuse will blow.

#### CAUSE:

------ The odometer stepper motor ribbon cable shorts against the speedometer circuit board. Only Fiero vehicles equipped with V6 engines are affected.

#### CORRECTION:

---------- Return defective odometers/speedometers to an authorized AC Spark Plug Service Center for repair. Vehicles after VIN GP207255 have been corrected.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.