TPS/TROUBLE CODE 22 INTERMITTENT TPS SWITCH. Pontiac Fiero 1984

For 1990-2009 cars

# TPS/TROUBLE CODE 22 INTERMITTENT TPS SWITCH

#### VEHICLES AFFECTED: 1984 Fiero

A stored code 22 could be caused by:

1. an intermittent TPS switch or 2. a poor connection at the TPS harness connector

If this condition occurs, replace the TPS switch with a new TPS kit, Part Number 17110648. The male TPS harness connector should be inspected for poor connections and the contact pins (male) should make sufficient contact to the TPS plug.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.