OTC MONITOR 85 SCAN TOOL INFORMATION. Pontiac Fiero 1985

For 1990-2009 cars

# OTC MONITOR 85 SCAN TOOL INFORMATION

1985 FIERO WITH 2.8L-PFI V6 ENGINE (VIN CODE 9)

Some technicians may be experiencing difficulty in using the OTC Monitor 85 Scan Tool model no. 3485* on Fieros with 2.8L - PFI V6 Engines (VIN Code 9). To properly use the Scan Tool on subject vehicles it is important that Monitor Code 14 (PONT 6PFI) be entered. Entering Code 13 (CHEV PFI) will result in erroneous readouts.

* "We believe this source and their equipment to be reliable. There may be additional manufacturers of such equipment. General Motors does not endorse, indicate any preference for or assume any responsibility for the products or equipment from these firms or for any such items which may be available from other sources."

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.