Reverse Brake Piston Removal. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

#### Tools Required

• | J 41681 Clutch Spring Compressor

• | J 23327 Clutch Spring Compressor

1. Remove the brake apply cover bolts.
2. Remove the brake apply cover.
3. Compress the reverse brake piston using the J 41681 and the J 23327 .
4. Remove the snap ring.
5. Cover the reverse brake piston with a clean cloth.
6. Slowly apply low pressure compressed air to the fluid passage B (2) while holding the fluid passage A (1) closed until the following components are forced out of the transmission:

• | The outer reverse brake piston

• | The reaction sleeve

• | The inner reverse brake piston

7. Remove the piston O-ring seals.