Automatic Transmission Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Cruise Control Actuator | RH Engine Compartment, near Strut Tower | Cruise Control Component Views in Cruise Control | --
Four Wheel Drive Low Switch | Top of Transfer Case | -- | --
Fuse Block 1 | RH Engine Compartment, front of Battery | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 1 - C1 (3 Cavities) | Main Harness to Fuse Block 1, below Fuse Block 1 | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 2 | Under LH I/P | Power and Grounding Component Views in Wiring Systems | --
Instrument Panel Cluster Assembly | LH I/P | Instrument Panel, Gages, and Console Component Views in Instrument Panel,Gauges,and Consol | --
Instrument Panel Cluster Assembly C1 (16 Terminals) | I/P Harness to I/P Cluster Assembly, behind I/P Cluster Assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel,Gauges,and Consol | --
Instrument Panel Cluster Assembly C3 (13 Terminals) | I/P Harness to I/P Cluster Assembly, behind I/P Cluster Assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel,Gauges,and Consol | --
Main Relay | Center I/P, behind Blower Speed Selector Switch | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Powertrain Control Module (PCM) | Under LH I/P, left of Steering Column | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Powertrain Control Module (PCM) - C1 (22 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Powertrain Control Module (PCM) - C3 (16 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Powertrain Control Module (PCM) - C4 (26 Cavities) | Main Harness to PCM, behind I/P left of Steering Column | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
Power/Normal Switch | In Center Console, right of Manual Selector Lever | -- | --
Shift Solenoid No. 1 | In Transmission, attached to Valve Body | -- | --
Shift Solenoid No. 2 | In Transmission, attached to Valve Body | -- | --
Stoplamp Switch | Under LH I/P, above Brake Pedal | Lighting Systems Component Views in Lighting Systems | --
Torque Converter Clutch (TCC) Solenoid | In Transmission, attached to Valve Body | -- | --
Transmission Range Switch | RH side of Transmission | -- | --
Vehicle Speed Sensor (VSS) | LH side of Transmission, in Adapter Case | -- | --
C100 (16 cavities) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views in Wiring Systems | --
C101 (16 Cavities) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views in Wiring Systems | --
C102 (4 Cavities) (Manual and Automatic Transmissions) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views in Wiring Systems | --
C103 (12 Cavities) (Manual and 4-Speed Transmissions) | Main Harness to Engine Harness, mounted to Bracket on Bulkhead, left of Front Wiper Motor | Harness Routing Views in Wiring Systems | --
C104 (9 Cavities) | Engine Harness to Transmission Harness, under Intake Manifold | Harness Routing Views in Wiring Systems | --
C106 (10 Cavities) | Engine Harness to Transmission Harness, RH rear Engine, under Intake Manifold | Harness Routing Views in Wiring Systems | --
C200 (22 Cavities) | Main Harness to I/P Harness, LH I/P near Fuse Block 2 | Harness Routing Views in Wiring Systems | --
C201 (16 Cavities) | Main Harness to I/P Harness, LH I/P near fuse Block 2 | Harness Routing Views in Wiring Systems | --
C213 (6 Cavities) | I/P Harness to Shift Illumination Jumper Harness, Center I/P | Harness Routing Views in Wiring Systems | --
G103 | RH Rear Engine Compartment mounted to Intake Manifold | Harness Routing Views in Wiring Systems | --
G200 | Behind LH I/P, above Fuse Block 2 | Harness Routing Views in Wiring Systems | --
P200 | LH Rear Engine Compartment on Bulkhead, near Brake Master Cylinder | Harness Routing Views in Wiring Systems | --
P201 | RH Rear Engine Compartment on Bulkhead, near Battery | Harness Routing Views in Wiring Systems | --
S107 | Engine Harness, Approximately 10 cm (3.93 in) from C104 breakout | -- | --
S108 | Transmission Harness, near 4WD Switch breakout | -- | --
S139 | Main Harness, approximately 10 cm (3.93 in) from Noise Suppressor Filter connector breakout | -- | --
S140 | Main Harness, approximately 6 cm (2.36 in) from Noise Suppressor Filter connector breakout | -- | --
S201 (4-Door) | I/P Harness, near the C211 breakout | Harness Routing Views in Wiring Systems | --
S208 | Main Harness, approximately 18 cm (7.08 in) from Ignition Switch connector breakout | Harness Routing Views in Wiring Systems | --
S204 | I/P Harness, near the C211 breakout | Harness Routing Views in Wiring Systems | --
S210 | Main Harness, approximately 12 cm (4.72 in) from Stoplamp Switch connector breakout | -- | --
S215 | Main Harness, near the Powertrain Control Module (PCM) connector C2 breakout | -- | --
S218 | Main harness, near G200 breakout | -- | --
S219 | Main Harness, approximately 10 cm (3.93 in) from Daytime Running Lamps (DRL) Control Module connector breakout | -- | --
S226 | I/P Harness, near the Radio breakout | Harness Routing Views in Wiring Systems | --
S230 | Main Harness, approximately 5 cm (1.96 in) from G300 breakout | Harness Routing Views in Wiring Systems | --
S234 | In Manual Selector Lever Harness | -- | --
S251 | Main Harness, approximately 5 cm (1.96 in) from Stoplamp Switch connector breakout | -- | --
S254 | Main Harness, approximately 10 cm (3.93 in) from G200 breakout | Harness Routing Views in Wiring Systems | --
S260 | Main Harness, approximately 4 cm (1.57 in) from Stoplamp Switch connector breakout | Harness Routing Views in Wiring Systems | --
S262 | Main Harness, approximately 8 cm (3.14 in) from Stoplamp Switch connector breakout | Harness Routing Views in Wiring Systems | --
S264 | Main Harness, approximately 18 cm (7.08 in) from Blower Speed Selector Switch connector breakout | Harness Routing Views in Wiring Systems | --
S272 | Main Harness, approximately 11 cm (4.33 in) from G200 breakout | Harness Routing Views in Wiring Systems | --
S276 | Main Harness, approximately 1 cm (0.39 in) from G200 breakout | -- | --
S288 | Main Harness, approximately 2 cm (0.78 in) from G200 breakout | -- | --
S294 | Main Harness, approximately 10 cm (3.93 in) from G200 breakout | Harness Routing Views in Wiring Systems | --
S295 | Main Harness, approximately 7 cm (2.75 in) from Blower Speed Selector Switch connector breakout | Harness Routing Views in Wiring Systems | --
S298 | Main Harness, approximately 2 cm (0.78 in) from G200 breakout | -- | --