Rear Side Door Inside Handle Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the screw and the inside handle (5) from the door.
2. Remove the rear side door inside handle rod from the handle (5).
3. Remove the inside handle (5) from the vehicle.

### Installation Procedure

1. Install the rear side door inside handle rod to the handle (5).
2. Install the rear side door inside handle (5) to the door. Secure the handle (5) with the screw.