Air Conditioning (A/C) Compressor Control Module Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Pull the instrument panel compartment out while pushing in the right and left stoppers.
2. Disconnect the A/C compressor control module electrical connector.
3. Remove the A/C compressor control module (2) from the evaporator case (1) by releasing the 2 lower lock tabs and sliding the compressor control module upward in order to disengage from the case.

### Installation Procedure

1. Install the A/C compressor control module (2) to the evaporator case (1). Slide the compressor control module downward and snap the compressor control module into place.
2. Connect the A/C compressor control module electrical connector.
3. Close the instrument panel compartment.