Antenna Diagnostic Check. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Lead-in Cable Resistance Values

Digital Multimeter probes at points: | Resistance measured in ohms
--- | ---
C and D | less than 1.0
C and B | infinite
C and G | infinite

### Antenna System Resistance Values

Ohmmeter probes at points: | Resistance measured in ohms
--- | ---
A and B | less than 0.15
A and E | less than 0.15
B and E | less than 0.15
A and C | infinite
B and C | infinite
B and D | infinite
A and D | infinite