Folding Top Rear Window Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Open the rear door.
2. Unfasten the corner flap of the folding top on the lower left side of the rear window frame in order to uncover the zipper pull ring (1).
3. Unfasten the corner flap of the folding top on the lower right side of the rear door.
4. Unzip the rear window (2) from the folding top.
5. Drape the rear window (2) down and rearward.
6. Pull the rear window and the frame rearward and remove from the vehicle.
7. If removing the rear window from the window frame, slide the window sideward from the frame.

### Installation Procedure

1. Install the rear window and frame to the vehicle.
2. Zip the rear window (2) to the canvas top.
3. Fasten the folding top corner flaps on the lower right and left sides of the rear window frame.