Fastener Tightening Specifications. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Hood Hinge-to-Body Bolts | 27 N·m | 20 lb ft
Hood Latch Retaining Bolts | 7 N·m | 5 lb ft
Hood Retaining Bolts | 27 N·m | 20 lb ft
Horn Mounting Bolt | 10 N·m | 89 lb in
Front Fender Bolts | 20 N·m | 15 lb ft
Front Upper Panel Bolts | 20 N·m | 15 lb ft
Front Wiper Arm Retaining Nuts | 20 N·m | 15 lb ft
Rocker Panel Front Trim Cover Nut | 15 N·m | 11 lb ft