Entertainment Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in Wiring Systems | --
LH Rear Speaker (2-Door) | LH rear quarter trim panel in front of the rear seat | Entertainment Component Views | --
LH Rear Speaker (4-Door) | LH rear quarter trim panel behind the rear seat | Entertainment Component Views | --
Radio | Center of the instrument panel | Entertainment Component Views | --
RH Front Speaker | RH top of the instrument panel near the windshield | Entertainment Component Views | --
RH Rear Speaker (2-Door) | RH rear quarter trim panel in front of the rear seat | Entertainment Component Views | --
RH Rear Speaker (4-Door) | RH rear quarter trim panel behind the rear seat | Entertainment Component Views | --
C200 (22 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C211 (16 Cavities) | Instrument panel harness to the floor harness, RH instrument panel near the A-pillar | Harness Routing Views in Wiring Systems | --
C301 (6 Cavities) (2-Door) | Floor harness to the sub-floor harness behind the LH rear passenger compartment trim panel | Harness Routing Views in Wiring Systems | --
G200 | Behind the LH instrument panel above fuse block 2 | Power and Grounding Component Views in Wiring Systems | --
S225 | Instrument panel harness approximately 12 cm (4.72 in) from the cigar lighter | Harness Routing Views in Wiring Systems | --
S226 | Instrument panel harness approximately at the radio breakout | Harness Routing Views in Wiring Systems | --
S230 | Main harness approximately 5 cm (1.96 in) from the G300 breakout | Harness Routing Views in Wiring Systems | --
S276 | Main harness approximately 1 cm (0.39 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --