Fastener Tightening Specifications. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Conditioning Compressor Mounting Bolts

- 8 mm Bolts

28 N·m

21 lb ft

- 10 mm Bolts

45 N·m

33 lb ft

Center Link-to-Pitman Arm Castle Nut | 55 N·m | 40 lb ft
Engine Skid Plate Bolts | 27 N·m | 20 lb ft
Pitman Arm Sector Shaft Nut | 130 N·m | 95 lb ft
Power Steering Gear Mounting and Pilot Bolts | 85 N·m | 61.5 lb ft
Power Steering Gear Pressure Hose Union Bolt | 40 N·m | 29 lb ft
Power Steering Pump Mounting Bolts | 30 N·m | 22 lb ft
Power Steering Pump Pressure Connector | 66 N·m | 48 lb ft
Power Steering Pump Pressure Switch | 18 N·m | 13.5 lb ft
Power Steering Pump Rear Cover/Cam Ring Bolts | 24 N·m | 17.5 lb ft
Power Steering Pump Suction Hose Connector Bolts | 10 N·m | 89 lb in