Electronic Brake Control Relay Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

The electronic brake control relay is located on the left hand side of the engine compartment, on the inner fender next to the hydraulic modulator.

1. Pull the relay (2) from the mounting bracket.
2. Disconnect the relay (2) from the relay harness connector.

### Installation Procedure

1. Connect the Relay (2) to the relay harness connector.
2. Install the Relay (2) to the mounting bracket.
3. Perform the Diagnostic System Check .