Fastener Tightening Specifications. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

#### Fastener Tightening Specifications

Application | Specification
--- | ---
Metric | English
Ball Stud Castle Nut | 58 N·m | 43 lb ft
Load Sensing Spring Bracket Bolts

- Minimum

18 N·m

13.5 lb ft

- Maximum

25 N·m

18 lb ft

Parking Brake Cable Nut and Bolt | 10 N·m | 89 lb in
Rear Suspension Support Mount Bolts | 50 N·m | 37 lb ft
Rear Suspension Upper Control Arm Nuts and Bolts | 90 N·m | 66 lb ft
Shock Absorber Locknut | 29 N·m | 21 lb ft
Shock Absorber Lower Bolt and Nut | 85 N·m | 63 lb ft
Shock Absorber Upper Retaining Nut | 29 N·m | 21 lb ft
Trailing Arm Front and Rear Nuts and Bolts | 90 N·m | 66 lb ft