Trim Height Specifications. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Table 1: | Trim Height Measurement Points
Table 2: | Trim Height Specifications
Table 3: | Trim Height Specifications
Table 4: | Trim Height Specifications

#### Trim Height Measurement Points

Application | Specification
--- | ---
Metric | English
2WD Folding Top

- Distance A

500 mm

19.70 in

- Distance B

500 mm

19.70 in

4WD Folding Top

- Distance A

500 mm

19.70 in

- Distance B

500 mm

19.70 in

2WD Four Door

- Distance A

500 mm

19.70 in

- Distance B

500 mm

19.70 in

4WD Four Door

- Distance A

500 mm

19.70 in

- Distance B

500 mm

19.70 in

#### Trim Height Specifications

(1) | Body
(1) | Body
(2) | Ground
(2) | Ground

#### Trim Height Specifications

Application | Specification
--- | ---
Metric | English
2WD Folding Top

- Trim Height J

282 mm

11.10 in

- Trim Height K

303 mm

11.93 in

4WD Folding Top

- Trim Height J

301 mm

11.85 in

- Trim Height K

322 mm

12.68 in

2WD Four Door

- Trim Height J

282 mm

11.10 in

- Trim Height K

303 mm

11.93 in

4WD Four Door

- Trim Height J

301 mm

11.85 in

- Trim Height K

322 mm

11.68 in

#### Front Suspension

(1) | Body
(2) | Strut
(3) | Coil Spring
(4) | Bump Stopper
(5) | Control Arm
(6) | Ball Stud
(7) | Wheel
(8) | Wheel Hub
(9) | Wheel Bearing
(10) | Steering Knuckle

#### Trim Height Specifications

Model | Clearance Z
--- | ---
Metric | English
2WD Folding Top | 91 mm | 3.60 in
4WD Folding Top | 91 mm | 3.60 in
2WD Four Door | 91 mm | 3.60 in
4WD Four Door | 91 mm | 3.60 in

#### Rear Suspension

(1) | Rear Suspension Upper Arm
(2) | Rear Coil Spring
(3) | Rear Shock Absorber
(4) | Rear Axle Housing
(5) | Trailing Arm

#### Trim Height Specifications

Model | Clearance D
--- | ---
Metric | English
2WD Folding Top | 212 mm | 8.35 in
4WD Folding Top | 212 mm | 8.35 in
2WD Four Door | 212 mm | 8.35 in
4WD Four Door | 212 mm | 8.35 in