Propeller Shaft Runout Specifications. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Application | Metric | English
--- | --- | ---
Aluminum Wheel

- Lateral Runout

0.762 mm

0.035 in

- Radial Runout

0.762 mm

0.030 in

Propeller Shaft Runout Specifications

- Center

0.80 mm

0.031 in

- Front

0.80 mm

0.031 in

- Rear

0.80 mm

0.031 in

Steel Wheel Runout

- Lateral Runout

1.14 mm

0.045 in

- Radial Runout

1.01 mm

0.040 in

Tire and Wheel Assembly (Radial and Lateral Runout)

- Off-Vehicle

1.27 mm

0.050 in

- On-Vehicle

1.52 mm

0.060 in