Standard Wheel/Column Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in Wiring Systems | --
Park/ Neutral Position (PNP) Switch (3-Speed Automatic Transmission) | RH side of the transmission | -- | --
Shift Lock Solenoid (Automatic Transmission) | Center console under the manual selector lever assembly | -- | --
Shift Lock Solenoid Capacitor (Automatic Transmission) | Center console under the manual selector lever assembly | -- | --
Stoplamp Switch | Under the LH instrument panel above the brake pedal | Lighting Systems Component Views in Lighting Systems | --
C100 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in Wiring Systems | --
C103 (12 Cavities) (Manual and 4-Speed Automatic Transmission) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in Wiring Systems | --
C106 (10 Cavities) (4-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views in Wiring Systems | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C213 (6 Cavities) | Instrument panel harness to the shift illumination | Harness Routing Views in Wiring Systems | --
G200 | Behind the LH instrument panel above fuse block 2 | Power and Grounding Component Views in Wiring Systems | --
P200 | LH rear engine compartment on the bulkhead near the brake master cylinder | Harness Routing Views in Wiring Systems | --
S208 | Main harness approximately 18 cm from the ignition switch connector breakout | Harness Routing Views in Wiring Systems | --
S228 | Main harness approximately 4 cm from the C212 breakout | Harness Routing Views in Wiring Systems | --
S230 | Main harness approximately 5 cm from the G300 breakout | Harness Routing Views in Wiring Systems | --
S234 (4-Speed Automatic Transmission) | In the manual selector lever harness | Harness Routing Views in Wiring Systems | --
S262 | Main harness approximately 8 cm from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --